d. Broadcast

e. switch1 makes 2 PDU copy

f.172.16.31.3

g. The Source and Destination MAC addresses are 000C.85CC.1DA7 >> 0060.7036.2849

h. switch1 makes 5 PDU copy

step 2

c.0060.7036.2849

d. When it doesn’t know the destination MAC address

part 2

c. 4 replies and 4 received

step 2

a.yes

b.yes

c.because devices connect to one port from access point

part 3

c. 172.16.31.1 Enter arp -d to clear the ARP table and switch to Simulation

e. 2

f. 172.16.31.1

g. в другой сети поэтому отправителем становится устройство выс уровня

step 2

zero

yes

it times out